## output to X <yes/no>
out_to_x no

## Create own window to draw <yes/no>
own_window no

## Print everything to console?
out_to_console yes

## Use double buffering (reduces flicker, not needed for console output)
double_buffer no

## Set to yes if you want Conky to be forked in the background
background no

## Update interval in seconds
update_interval 1.0

## This is the number of times Conky will update before quitting.
## Set to zero to run forever.
total_run_times 0

## How strict should if_up be when testing an interface for being up?
## The value is one of up, link or address, to check for the interface
## being solely up, being up and having link or being up, having link
## and an assigned IP address.
if_up_strictness address


## Force UTF8? note that UTF8 support required XFT
override_utf8_locale yes

use_spacer left

TEXT
%{c} load: ${loadavg 1} ${loadavg 2} ${loadavg 3} | ram: ${memperc}% | swap: ${swapperc} | processes: ${processes} | ${if_up wlan0} wlan:${wireless_link_qual_perc wlan0}% ${wireless_essid wlan0} ↓${downspeed wlan0} ↑${upspeed wlan0} |$endif ${if_up enp0s25:} lan: ↓${downspeed wlan0} ↑${upspeed wlan0} |$endif bat ${exec $HOME/.config/herbstluftwm/conky-bat/index.js}
